Noritake 则武公司 网址：http://www.noritake.co.jp/china/

Grinding Wheel 砂轮

Tool No. 工厂号WUXI KOYO Mfg. No. 生产批号

Item No. 产品编号

|  |  |  |
| --- | --- | --- |
| Abrasive磨料 | GritSize 粒度 | Grade 硬度 |
| A 氧化铝 | 0150 | R |

|  |  |  |
| --- | --- | --- |
| Structure 密度 | Bond 结合剂 | Shape 形状 |
| 3 | R40 | 1 |

Size 尺寸

Max Operating Speed 最大转速

Use within 4 years from the manufacturing date 从生产之日起4年内使用

WARNING 警告

1. Always wear eye protection that complies with current ANSI Standard B7-1

佩戴符合ANSI B7-1标准的保护面罩

1. Never exceed maximum r.p.m rating.
2. Never use without proper safety guarding.
3. Always use equal size, recessed flanges that are 1/3 the diameter of the grinding wheel.
4. Never force wheel onto machine sprindle or overtighten nut.
5. Store carefully, do not drop.
6. Always visually inspect before mounting.
7. Never use wheel when damage is suspected.
8. Stand clear on initial start up.
9. Never grind on side of wheel
10. Observe ANSI B7-1, OSHA or your national safety regulations. FAILURE TO HEED ALL WARNINGS AND INSTRUCTIONS COULD RESULT IN SERIOUS BODILY INJURY.

NORIKATE Co., LIMITED

Noritake, Nagoya, Japan

Made in Japan